{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["招标控价"],"not_rendered":{"external_links":16,"defined_names":108},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"招标控价","index":0,"n_rows":100,"n_cols":9,"rows_kept":100,"merged":[[0,0,0,8],[99,0,99,8]],"flags":["formulas_cached_only"]}
["工程量清单报价"]
["序号","项目名称","项目特征","工作内容","单位","工程量","全费用综合单价(元)","合计（元）","备注"]
[null,"园建"]
["一","土方"]
[1,"机械挖土方","1.土壤类别：二、三类土\n2.挖土深度：3米以内\n3.综合运距：1km,土方就场地内用于回填消化\n4.须按照施工图设计要求标高进行\n5.按符合图纸要求的合格施工内容，按图示开挖面积乘以挖土深度以天然密实体积计量","放线、开挖、运输、将土方倾倒至甲方指定的场内需回填范围内、碾压、整平、压实","m3",{"v":19082.97475,"d":"19082.97"},null,null,"含机械费"]
[2,"人工挖沟槽（坑）土方","1.土壤类别：二、三类土\n2.挖土深度：2米以内\n3.综合运距：1km,土方就场地内用于回填消化，\n4.须按照施工图设计要求标高进行\n5.按符合图纸要求的合格施工内容，按图示开挖面积乘以挖土深度以天然密实体积计量","人工挖沟槽（坑）土方、修整沟槽（坑）底、边坡等","m3",{"v":150,"d":"150.00"}]
[3,"基础土方整形、平整压实","1.原状土密实度要求：≥0.90；\n2.机械原土夯实；         \n3.按符合图纸要求的合格施工内容，按图示尺寸以面积计量","广场、道路等30cm之内基础整形、平整","m2",{"v":30920.401,"d":"30920.40"},null,null,"含机械费"]
["二","道路、广场、停车场基层"]
[1,"园路灰土垫层","1.垫层材料种类：三七灰土；\n2.完成面标高误差2cm以内\n3.按符合图纸要求的合格施工内容，按图示尺寸或实际施工尺寸以两者尺寸较小的体积计量","灰土拌合、场内运输、摊铺、找平、压实等","m3",{"v":3762.823,"d":"3762.82"},null,null,"含机械费\n材料甲供"]
[2,"碎石垫层","1.垫层材料种类：碎石；\n2.完成面标高误差2cm以内\n3.按符合图纸要求的合格施工内容，按图示尺寸或实际施工尺寸以两者尺寸较小的体积计量","碎石场内运输、摊铺、找平、压实等","m3",3650.02,null,null,"含机械费\n材料甲供"]
[3,"砖渣垫层","1.垫层材料种类：碎石；\n2.完成面标高误差2cm以内\n3.按符合图纸要求的合格施工内容，按图示尺寸或实际施工尺寸以两者尺寸较小的体积计量","砖渣场内运输、摊铺、找平、压实等","m3",854.72,null,null,"含机械费\n材料甲供"]
[4,"砂垫层","1.垫层材料种类：砂；\n2.按符合图纸要求的合格施工内容，按图示尺寸或实际施工尺寸以两者尺寸较小的体积计量","砂场内运输、摊铺、找平、压实等","m3",{"v":131.5,"d":"131.50"},null,null,"含机械费\n材料甲供"]
[5,"非泵送混凝土垫层","1.垫层材料种类：非泵送混凝土;\n2.完成面标高误差1cm以内；     \n3.按符合图纸要求的合格施工内容，按图示尺寸或实际施工尺寸以两者尺寸较小的体积计量","混凝土场内运输、浇筑、振捣、找平、切缝、清扫现场、养护成品保护等","m3",920.61,null,null,"材料甲供"]
[6,"泵送混凝土垫层","1.垫层材料种类：泵送混凝土;\n2.完成面标高误差1cm以内；     \n3.按符合图纸要求的合格施工内容，按图示尺寸或实际施工尺寸以两者尺寸较小的体积计量","混凝土场内运输、浇筑、振捣、找平、切缝、清扫现场、养护、成品保护等","m3",2025.07,null,null,"材料甲供"]
[7,"垫层模板","1.尺寸：按照实际施工需要切割\n2.按与混凝土接触面计量模板面积","模板制作、安拆及模板堆放地与使用区域之间运输、归集、码放、场内运输","m2",919.85,null,null,"材料甲供"]
["三","结构工程"]
[1,"小型砖砌体","1.砖品种、规格、强度等级:粉煤灰砖\n2.墙体类型:排水沟、坐凳、花池、园林小品等砖砌体（不含围墙）\n3.砂浆强度等级、配合比:M5水泥砂浆\n4.按符合图纸要求的合格施工内容，按图示尺寸以体积计量","基层清理、砂浆调制、砌砖砌体、场内材料运输、养护、清扫现场、成品保护等","m3",{"v":346,"d":"346.00"},null,null,"材料甲供"]
[2,"墙面一般抹灰","1.厚度:20mm\n2.砂浆种类:1：2水泥砂浆\n3.按符合图纸要求的合格施工内容，按图示尺寸以面积计量","基层清理、砂浆调制、墙面抹灰、清扫现场、成品保护等","m2",{"v":240,"d":"240.00"},null,null,"材料甲供"]
[3,"钢筋制安","1.钢筋种类、规格:综合\n2.按符合图纸要求的合格施工内容，以图示尺寸以吨计量","场内运输、调直、折弯、制作、安装等，包含钢筋调直机、切断机等机械费用","t",45.48,null,null,"材料甲供"]
[4,"结构混凝土（泵送）","1.混凝土种类:泵送\n2.结构类型:柱、梁、墙、板等\n3.按符合图纸要求的合格施工内容，按图示尺寸以体积计量","混凝土场内运输、振捣、浇筑、养护、清扫现场、成品保护","m3",{"v":210,"d":"210.00"},null,null,"材料甲供"]
[5,"结构混凝土（非泵送）","1.混凝土种类:非泵送\n2.结构类型:柱、梁、墙、板等\n3.按符合图纸要求的合格施工内容，按图示尺寸以体积计量","混凝土场内运输、振捣、浇筑、养护清扫现场、成品保护等，包含混凝土震动器等机械费用和De100排水管（间距2m）预埋费用","m3",{"v":58,"d":"58.00"},null,null,"材料甲供"]
[6,"结构模板（基础、柱、梁、墙、板等结构）","1.尺寸：按照实际施工需要切割\n2.按与混凝土接触面计量模板面积","模板制作、安拆及模板堆放地与使用区域之间运输、归集、码放、场内运输","m2",{"v":240,"d":"240.00"},null,null,"材料甲供"]
["四","装饰墙面工程"]
[1,"石材饰面","1.20mm厚石材贴面\n2.20厚1:3水泥砂浆           \n3.材料倒运，综合运距1km；\n4.按符合图纸要求的合格施工内容，以图示面积计量","基层清理、砂浆调制、运输，材料场内运输、铺贴、清扫现场、成品保护等","m2",{"v":263,"d":"263.00"},null,null,"材料甲供"]
[2,"石材压顶","1.50/80/100mm厚石材压顶\n2.20厚1:3水泥砂浆           \n3.材料倒运，综合运距1km；\n4.按符合图纸要求的合格施工内容，按图示尺寸以面积计量","基层清理、砂浆调制、运输，材料场内运输、铺贴、清扫现场、成品保护等","m2",{"v":65,"d":"65.00"},null,null,"材料甲供"]
["五","地面铺装工程"]
[1,"碎石铺面","1.面层材料：80厚粒径Φ20-30浅灰色碎石\n2.按符合图纸要求的合格施工内容，按图示尺寸以面积计量","基层清理、砂浆调制、运输，材料场内运输、回填、摊铺、压实、清扫现场、成品保护等","m2",{"v":848,"d":"848.00"},null,null,"材料甲供"]
[2,"花岗岩铺装","1.面层材料：规格板花岗岩（厚3.1-5cm）                   \n2.结合层厚度：30厚1:3干硬性水泥砂浆结构层\n3.按符合图纸要求的合格施工内容，按图示尺寸以面积计量","基层清理、砂浆调制、运输，材料场内运输、铺贴、清扫现场、成品保护等","m2",1998.59,null,null,"材料甲供"]
[3,"花岗岩台阶铺装","1.面层材料：50厚花岗岩台阶\n2.结合层厚度：30厚1:2.5水泥砂浆结构层                           \n3.按符合图纸要求的合格施工内容，按图示尺寸以水平投影面积计算","基层清理、砂浆调制、运输，材料场内运输、铺贴、清扫现场、成品保护等","m2",123.88,null,null,"材料甲供"]
[4,"小料石铺装（收边或分隔条）","1.面层材料：100X100X100（50）厚黑色小料石\n2.结合层厚度：30厚1:2.5水泥砂浆结构层\n3.按符合图纸要求的合格施工内容，按图示尺寸以面积计量","基层清理、砂浆调制、运输，材料场内运输、铺贴、清扫现场、成品保护等","m2",302.04,null,null,"材料甲供"]
[5,"停车场植草格","1.面层材料：70厚植草格\n2.结合层厚度：30厚砂垫层\n3.按符合图纸要求的合格施工内容，按图示尺寸以面积计量","基层清理、材料场内运输、砂回填、摊铺、找平、压实、植草格切割、铺设、连接扣件、格内土回填、清扫现场、成品保护等","m2",2240.96,null,null,"材料甲供"]
[6,"花岗岩道牙","1.路牙材料种类、规格:600x120x250厚中国灰麻机切面花岗岩道牙\n2.砂浆强度等级：30厚1:3水泥砂浆粘结层\n3.靠背混凝土浇筑\n4.按符合图纸要求的合格施工内容，按图示尺寸以长度计量","基层清理、砂浆调整、石材切割、材料运输、安装 、勾缝、护肩、扫缝、清扫现场、成品保护等","m",{"v":3527.8,"d":"3527.80"},null,null,"材料甲供"]
[7,"混凝土道牙","1.路牙材料种类、规格:150x300x600预制混凝土立(平)道牙\n2.砂浆强度等级：30厚1:3水泥砂浆粘结层\n3.靠背混凝土浇筑\n4.按符合图纸要求的合格施工内容，按图示尺寸以长度计量","基层清理、砂浆调整、预制混凝土切割、材料运输、安装 、勾缝、护肩、扫缝、清扫现场、成品保护等","m",1307.39,null,null,"材料甲供"]
[null,"小计"]
[null,"水电"]
["一","给水工程"]
[1,"给水管","1.材质：PE管\n2.规格：DN32\n3.连接方式：热熔连接\n4.按符合图纸要求的合格施工内容，按图示尺寸以长度计量","场内搬运、外观检查、切管、热熔、上管件、调直、水压试验等","m",{"v":100,"d":"100.00"},null,null,"材料甲供"]
[2,"给水管","1.材质：PE管\n2.规格：DN40\n3.连接方式：热熔连接\n4.按符合图纸要求的合格施工内容，按图示尺寸以长度计量","场内搬运、外观检查、切管、热熔、上管件、调直、水压试验等","m",{"v":100,"d":"100.00"},null,null,"材料甲供"]
[3,"给水管","1.材质：PE管\n2.规格：De50\n3.连接方式：热熔连接\n4.按符合图纸要求的合格施工内容，按图示尺寸以长度计量","场内搬运、外观检查、切管、热熔、上管件、调直、水压试验等","m",{"v":3112,"d":"3112.00"},null,null,"材料甲供"]
[4,"给水管","1.材质：PE管\n2.规格：De63\n3.连接方式：热熔连接\n4.按符合图纸要求的合格施工内容，按图示尺寸以长度计量","场内搬运、外观检查、切管、热熔、上管件、调直、水压试验等","m",{"v":665,"d":"665.00"},null,null,"材料甲供"]
[5,"给水管","1.材质：PE管\n2.规格：DN80\n3.连接方式：热熔连接\n4.按符合图纸要求的合格施工内容，按图示尺寸以长度计量","场内搬运、外观检查、切管、热熔、上管件、调直、水压试验等","m",{"v":150,"d":"150.00"},null,null,"材料甲供"]
[6,"给水管","1.材质：PE管\n2.规格：De110\n3.连接方式：热熔连接\n4.按符合图纸要求的合格施工内容，按图示尺寸以长度计量","场内搬运、外观检查、切管、热熔、上管件、调直、水压试验等","m",{"v":3558,"d":"3558.00"},null,null,"材料甲供"]
[7,"给水管","1.材质：PE管\n2.规格：DN160\n3.连接方式：热熔连接\n4.按符合图纸要求的合格施工内容，按图示尺寸以长度计量","场内搬运、外观检查、切管、热熔、上管件、调直、水压试验等","m",{"v":600,"d":"600.00"},null,null,"材料甲供"]
[8,"过路钢管","1.材质：镀锌钢管\n2.规格：DN100\n3.连接方式：焊接\n4.按符合图纸要求的合格施工内容，按图示尺寸以长度计量","场内搬运、管材防腐、检查及清扫管材、切管、套丝、上管件、管道及管件安装、丝口刷漆","m",{"v":266,"d":"266.00"},null,null,"材料甲供"]
[9,"循环水管","1.材质：热镀锌钢管\n2.规格：De160\n3.连接方式：焊接\n4.按符合图纸要求的合格施工内容，按图示尺寸以长度计量","场内搬运、管材防腐（三油两布）、检查及清扫管材、切管、套丝、上管件、管道及管件安装、丝口刷漆、水压试验、水冲洗","m",{"v":455,"d":"455.00"},null,null,"材料甲供"]
[10,"循环泵","1.型号及规格：100WQ100-15-7.5\n流量100m³/小时，扬程15米，7.5KW\n2.按符合图纸要求的合格施工内容，按图示尺寸以台计量","施工准备, 设备、材料及工、机具搬运, 设备开箱、点件、外观检查、基础施工, 设备找正、调平、精平、焊接、固定、灌浆、单机试运转","台",{"v":1,"d":"1.00"},null,null,"材料甲供"]
[11,"循环泵\n","1.型号及规格：100WQ80-10-4\n流量80m³/小时，扬程10米，4KW\n2.按符合图纸要求的合格施工内容，按图示尺寸以台计量","施工准备, 设备、材料及工、机具搬运, 设备开箱、点件、外观检查、基础施工, 设备找正、调平、精平、焊接、固定、灌浆、单机试运转","台",{"v":1,"d":"1.00"},null,null,"材料甲供"]
[12,"电磁阀","1.材质：铜质\n2.规格：DN50\n3.按符合图纸要求的合格施工内容，按图示以个数计量","阀门安装、调试等","个",{"v":4,"d":"4.00"},null,null,"材料甲供"]
[13,"闸阀","1.材质：铜质\n2.规格：De63\n3.按符合图纸要求的合格施工内容，按图示以个数计量","阀门安装、调试等","个",{"v":4,"d":"4.00"},null,null,"材料甲供"]
[14,"闸阀","1.材质：铜质\n2.规格：DN80\n3.按符合图纸要求的合格施工内容，按图示以个数计量","阀门安装、调试等","个",{"v":0,"d":"0.00"},null,null,"材料甲供"]
[15,"闸阀","1.材质：铜质\n2.规格：DN100\n3.按符合图纸要求的合格施工内容，按图示以个数计量","阀门安装、调试等","个",{"v":4,"d":"4.00"},null,null,"材料甲供"]
[16,"闸阀","1.材质：铜质\n2.规格：De160\n3.按符合图纸要求的合格施工内容，按图示以个数计量","阀门安装、调试等","个",{"v":1,"d":"1.00"},null,null,"材料甲供"]
[17,"可曲挠橡胶接头","1.位置：水表井内\n2.规格：DN100\n3.按符合图纸要求的合格施工内容，按图示以个数计量","阀门安装、调试等","个",{"v":1,"d":"1.00"},null,null,"材料甲供"]
[18,"止回阀","1.位置：水表井内\n2.规格：DN100\n3.按符合图纸要求的合格施工内容，按图示以个数计量","阀门安装、调试等","个",{"v":1,"d":"1.00"},null,null,"材料甲供"]
[19,"水表","1.位置：水表井内\n2.规格：DN100\n3.按符合图纸要求的合格施工内容，按图示以个数计量","阀门安装、调试等","个",{"v":2,"d":"2.00"},null,null,"材料甲供"]
[20,"截止阀DN25","1.材质：铜质\n2.规格：DN25\n3.按符合图纸要求的合格施工内容，按图示以个数计量","阀门安装、调试等","个",{"v":2,"d":"2.00"},null,null,"材料甲供"]
[21,"取水阀","1.规格：DN25\n2.按符合图纸要求的合格施工内容，按图示以个数计量","连接管安装，取水阀安装、调试，阀箱安装等","个",{"v":149,"d":"149.00"},null,null,"材料甲供"]
[22,"阀门井","1.尺寸：Φ1200，详见02S515-12\n2.按符合图纸要求的合格施工内容，按图示以座计量","砂浆拌合、砌砖、刮缝, 钢筋制安, 模板制安、拆除、清理, 混凝土浇筑、振捣、养护, 抹防水、防潮层, 井盖安装, 材料运输","座",{"v":8,"d":"8.00"},null,null,"材料甲供"]
[23,"水表井","1.尺寸：2150*1100，详见05S502\n2.按符合图纸要求的合格施工内容，按图示以座计量","砂浆拌合、砌砖、刮缝, 钢筋制安, 模板制安、拆除、清理, 混凝土浇筑、振捣、养护, 抹防水、防潮层, 井盖安装, 材料运输","座",{"v":2,"d":"2.00"},null,null,"材料甲供"]
[24,"管沟土方","1.土壤类别：三类土\n2.挖土深度：1米以内\n3.综合运距：就近搁置\n4.须按照施工图设计要求标高进行\n5.按符合图纸要求的合格施工内容，按图示及说明以天然密实体积计量","挖土，将土堆放在沟、槽周边,清理机下余土；清理边坡,工作面内人工排水等辅助性工作；就地取土、回填土、按照设计及规范要求夯填土、清理 ","m3",{"v":3271.7999999999997,"d":"3271.80"},null,null,"含机械费"]
["二","排水工程"]
[1,"排水管","1.材质：双壁波纹管\n2.规格：DN300\n3.连接方式：胶圈连接\n4.按符合图纸要求的合格施工内容，按图示尺寸以长度计量","场内搬运、外观检查、切管、管材及管件连接、调直、试验等","m",{"v":420,"d":"420.00"},null,null,"材料甲供"]
[2,"排水管","1.材质：双壁波纹管\n2.规格：DN200\n3.连接方式：胶圈连接\n4.按符合图纸要求的合格施工内容，按图示尺寸以长度计量","场内搬运、外观检查、切管、管材及管件安装、调直、试验等","m",{"v":243,"d":"243.00"},null,null,"材料甲供"]
[3,"排水管","1.材质：渗水管\n2.规格：RCP-Y15G \n3.连接方式：粘接\n4.按符合图纸要求的合格施工内容，按图示尺寸以长度计量","场内搬运、外观检查、切管、管材安装、调直、试验等","m",{"v":2219,"d":"2219.00"},null,null,"材料甲供"]
[4,"排水检查井","1.规格：02S515-12\n2.按符合图纸要求的合格施工内容，按图示以座计量","人工清底，井座砌筑、井盖安装，连接管材等","座",{"v":21,"d":"21.00"},null,null,"材料甲供"]
[5,"雨水口","1.规格：95S517-3\n3.按符合图纸要求的合格施工内容，按图示以座计量","人工清底，井座砌筑、井盖安装，连接管材等","座",{"v":17,"d":"17.00"},null,null,"材料甲供"]
[6,"管沟土方","1.土壤类别：三类土\n2.挖土深度：1.5米以内\n3.综合运距：就近搁置\n4.须按照施工图设计要求标高进行\n5.按符合图纸要求的合格施工内容，按图示及说明以天然密实体积计量","挖土，将土堆放在沟、槽周边,清理机下余土；清理边坡,工作面内人工排水等辅助性工作；就地取土、回填土、按照设计及规范要求夯填土、清理 ","m3",{"v":1296.9,"d":"1296.90"},null,null,"含机械费"]
[7,"管沟垫层回填","1.垫层类别：砂\n2.按符合图纸要求的合格施工内容，按图示及说明以天然密实体积计量","材料倒运，管沟垫层砂、石屑等回填，回填料顶层标高控制及平整","m3",112.56,null,null,"含机械费\n材料甲供"]
["三","电气工程"]
[1,"景观照明配电箱","1.名称:配电箱700*1500*400（详见图纸）\n2.型号、规格:按系统定制(防护等级IP54）\n3.基础形式、材质、规格:混凝土基础\n4.接线极材质、规格:50*5热镀锌角钢，长2.5m，间距5m\n5.接地线材质、规格:40*4热镀锌扁钢\n6.安装形式:落地安装\n7.包含独立接地装置调试\n8.按符合图纸要求的合格施工内容，按图示以座计量","电箱基础土方开挖、回填、基础支模浇筑、开箱、清扫、检查、测位、划线、钻孔、装螺栓、本体安装、盘内整理、接线、接地、补漆","台",{"v":6,"d":"6.00"},null,null,"材料甲供"]
[2,"水泵控制箱 ","1.名称:水泵控制箱700*1500*400 （详见图纸）\n2.型号、规格:按系统定制(防护等级IP54）\n3.基础形式、材质、规格:C20混凝土基础\n4.接线极材质、规格:50*5热镀锌角钢，长2.5m，间距5m\n5.接地线材质、规格:40*4热镀锌扁钢\n6.安装形式:落地安装\n7.包含独立接地装置调试\n8.按符合图纸要求的合格施工内容，按图示以座计量","电箱基础土方开挖、回填、基础支模浇筑、开箱、清扫、检查、测位、划线、钻孔、装螺栓、本体安装、盘内整理、接线、接地、补漆","台",{"v":2,"d":"2.00"},null,null,"材料甲供"]
[3,"电力电缆","1.型号、规格:YJV-22-4*25\n2.材质:铜芯\n3.敷设方式、部位:电缆沟直埋\n4.按符合图纸要求的合格施工内容，按图示尺寸以长度计量","清理沟槽、敷设、锯断、收线盘、测量绝缘电阻、临时封头、挂标牌","m",{"v":663,"d":"663.00"},null,null,"材料甲供"]
[4,"电力电缆","1.型号、规格:YJV-22-4*10\n2.材质:铜芯\n3.敷设方式、部位:电缆沟直埋\n4.按符合图纸要求的合格施工内容，按图示尺寸以长度计量","清理沟槽、敷设、锯断、收线盘、测量绝缘电阻、临时封头、挂标牌","m",{"v":1024,"d":"1024.00"},null,null,"材料甲供"]
[5,"电力电缆","1.型号、规格:YJV-22-4*16\n2.材质:铜芯\n3.敷设方式、部位:电缆沟直埋\n4.按符合图纸要求的合格施工内容，按图示尺寸以长度计量","清理沟槽、敷设、锯断、收线盘、测量绝缘电阻、临时封头、挂标牌","m",{"v":353,"d":"353.00"},null,null,"材料甲供"]
[6,"电力电缆","1.型号、规格:YJV-2*4\n2.材质:铜芯\n3.敷设方式、部位:穿管敷设\n4.按符合图纸要求的合格施工内容，按图示尺寸以长度计量","清理沟槽、敷设、锯断、收线盘、测量绝缘电阻、临时封头、挂标牌","m",{"v":3325,"d":"3325.00"},null,null,"材料甲供"]
[7,"电力电缆","1.型号、规格:YJV-2*10\n2.材质:铜芯\n3.敷设方式、部位:穿管敷设\n4.按符合图纸要求的合格施工内容，按图示尺寸以长度计量","清理沟槽、敷设、锯断、收线盘、测量绝缘电阻、临时封头、挂标牌","m",{"v":5167,"d":"5167.00"},null,null,"材料甲供"]
[8,"电力电缆","1.型号、规格:YJV-3*6\n2.材质:铜芯\n3.敷设方式、部位:穿管敷设\n4.按符合图纸要求的合格施工内容，按图示尺寸以长度计量","清理沟槽、敷设、锯断、收线盘、测量绝缘电阻、临时封头、挂标牌","m",{"v":212,"d":"212.00"},null,null,"材料甲供"]
[9,"电力电缆","1.型号、规格:YJV-4*6\n2.材质:铜芯\n3.敷设方式、部位:穿管敷设\n4.按符合图纸要求的合格施工内容，按图示尺寸以长度计量","清理沟槽、敷设、锯断、收线盘、测量绝缘电阻、临时封头、挂标牌","m",{"v":49,"d":"49.00"},null,null,"材料甲供"]
[10,"电力电缆","1.型号、规格:YJV-4*4\n2.材质:铜芯\n3.敷设方式、部位:穿管敷设\n4.按符合图纸要求的合格施工内容，按图示尺寸以长度计量","清理沟槽、敷设、锯断、收线盘、测量绝缘电阻、临时封头、挂标牌","m",{"v":88,"d":"88.00"},null,null,"材料甲供"]
[11,"电气配管","1.名称:电缆保护管\n2.材质:PVC\n3.规格:De50\n4.敷设方式:直埋\n5.按符合图纸要求的合格施工内容，按图示尺寸以长度计量","测位、断管、配管、固定、连接管件","m",{"v":5167,"d":"5167.00"},null,null,"材料甲供"]
[12,"电气配管","1.名称:电缆保护管\n2.材质:PVC\n3.规格:De32\n4.敷设方式:直埋\n5.按符合图纸要求的合格施工内容，按图示尺寸以长度计量","测位、断管、配管、固定、连接管件","m",{"v":3325,"d":"3325.00"},null,null,"材料甲供"]
[13,"庭院灯1","1.型号规格:30W H=3m\n2.防水防尘等级：IP65\n3.按符合图纸要求的合格施工内容，按图示以套计量","灯基础土方开挖、回填、基层素土夯实、基础支模浇筑、接线、电缆头连接、灯具安装、调试等","套",{"v":135,"d":"135.00"},null,null,"材料甲供"]
[14,"庭院灯2","1.型号规格:30W H=3m\n2.防水防尘等级：IP65\n3.按符合图纸要求的合格施工内容，按图示以套计量","灯基础土方开挖、回填、基层素土夯实、基础支模浇筑、接线、电缆头连接、灯具安装、调试等","套",{"v":38,"d":"38.00"},null,null,"材料甲供"]
[15,"路灯","1.型号规格:150W H=6m\n2.防水防尘等级：IP65\n3.按符合图纸要求的合格施工内容，按图示以套计量","灯基础土方开挖、回填、基层素土夯实、基础支模浇筑、接线、电缆头连接、灯具安装、调试等","套",{"v":72,"d":"72.00"},null,null,"材料甲供"]
[16,"草坪灯","1.型号规格:12W H=0.6m\n2.防水防尘等级：IP65\n3.按符合图纸要求的合格施工内容，按图示以套计量","灯基础土方开挖、回填、基层素土夯实、基础支模浇筑、接线、电缆头连接、灯具安装、调试等","套",{"v":24,"d":"24.00"},null,null,"材料甲供"]
[17,"单侧龟壳灯","1.型号规格:12W H=0.6m\n2.防水防尘等级：IP65\n3.按符合图纸要求的合格施工内容，按图示以套计量                             ","灯基础土方开挖、回填、基层素土夯实、基础支模浇筑、接线、电缆头连接、灯具安装、调试等","套",{"v":37,"d":"37.00"},null,null,"材料甲供"]
[18,"射树灯","1.型号规格:5W\n2.防水防尘等级：IP65\n3.按符合图纸要求的合格施工内容，按图示以套计量","灯基础土方开挖、回填、基层素土夯实、基础支模浇筑、接线、电缆头连接、灯具安装、调试等","套",{"v":73,"d":"73.00"},null,null,"材料甲供"]
[19,"地埋灯","1.型号规格:5W\n2.防水防尘等级：IP65\n3.按符合图纸要求的合格施工内容，按图示以套计量","灯基础土方开挖、回填、基层素土夯实、基础支模浇筑、接线、电缆头连接、灯具安装、调试等","套",{"v":75,"d":"75.00"},null,null,"材料甲供"]
[20,"水下灯","1.型号规格:5W\n2.防水防尘等级：IP65\n3.按符合图纸要求的合格施工内容，按图示以套计量","灯基础土方开挖、回填、基层素土夯实、基础支模浇筑、接线、电缆头连接、灯具安装、调试等","套",{"v":3,"d":"3.00"},null,null,"材料甲供"]
[21,"变压器","1.型号规格:220/12V 100VA\n2.防水防尘等级：IP65\n3.按符合图纸要求的合格施工内容，按图示以套计量                             ","变压器安装、调试等","套",{"v":1,"d":"1.00"},null,null,"材料甲供"]
[22,"接地级","1.材质、规格：2.5米的50*5热镀锌角钢\n2.按符合图纸要求的合格施工内容，按图示尺寸以根计量                             ","尖端加工、卡子制作、接地极打入、焊接刷油","根",{"v":51,"d":"51.00"},null,null,"材料甲供"]
[23,"接地母线","1.材质、规格：直径8镀锌圆钢\n2.按符合图纸要求的合格施工内容，按图示尺寸以根计量                             ","平直、断料、测位、钻孔、卡子制作、埋卡子、焊接、固定、刷油等","m",{"v":8704,"d":"8704.00"},null,null,"材料甲供"]
[24,"铺砂盖砖","1.位置：主电缆沟槽\n2.按符合图纸要求的合格施工内容，按图示尺寸以长度计量","材料倒运、沟槽清理、电缆沟铺砂盖砖","m",{"v":2040,"d":"2040.00"},null,null,"含机械费\n材料甲供"]
[25,"管沟土方","1.土壤类别：三类土\n2.挖土深度：1米以内\n3.综合运距：就近搁置\n4.须按照施工图设计要求标高进行\n5.按符合图纸要求的合格施工内容，按图示及说明以天然密实体积计量","挖土，将土堆放在沟、槽周边,清理机下余土；清理边坡,工作面内人工排水等辅助性工作；就地取土、回填土、按照设计及规范要求夯填土、清理","m3",{"v":3916.8,"d":"3916.80"},null,null,"含机械费"]
[null,"小计"]
[null,"其他"]
[1,"大工","工作时间为9个小时",null,"工日",{"v":100,"d":"100.00"}]
[2,"小工","工作时间为9个小时",null,"工日",{"v":100,"d":"100.00"}]
[null,"合计",{"$nulls":5},{"v":0,"d":"0.00"}]
["注：1.全费用综合单价包含完成分部分项工程项目的全部费用价格（税金按9%考虑），其组成包括但不限于人工费（包括人员加班工资、差旅及窝工费、承包人供应材料保管费等）、材料运输、卸车及二次搬运费、二次或者多次进出场费、已完工项目成品保护措施费、机械使用费及进出场安拆费、耗材费、试验及工程检测费用、管理费、利润、风险、规费、税金以及夜间照明、防尘、施工便道、安全文明（标识标牌的制作、购买及安装，绿网的掀盖，现场安全人员管理）、赶工等措施费用。交叉施工影响及配合费用，施工人员的食宿费、劳保费用、办公费、生活生产水电费、保险费也包含在报价里。\n2.结算量以招标人现场负责人、成本专员、施工员联签的现场计量工程量计算，最终结算以公司内审部审计后金额为准。\n3.清单计量规格实行《2013年工程量清单计量规范》。\n4.验收规范：以设计说明中验收规范为准 。                                         \n5.以上报价按9%的增值税税金报价，签订合同时按实际税点调整合同单价。           \n6.以上清单中场内运输距离：1km以内综合考虑。"]