{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["附件","Sheet3"],"not_rendered":{"images":3,"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"附件","index":0,"n_rows":27,"n_cols":5,"rows_kept":27,"merged":[[0,0,0,3],[1,2,1,3],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[9,2,9,3],[10,2,10,3],[11,2,11,3],[12,2,12,3],[13,2,13,3],[14,2,14,3],[15,2,15,3],[16,2,16,3],[17,2,17,3],[18,2,18,3],[19,2,19,3],[20,0,20,4],[22,0,22,4],[24,4,26,4]],"flags":["formulas_cached_only"]}
["附表                                路灯参数"]
["序号","型号","单晶",null,"单晶"]
[1,"光伏板功率","60W",null,"130W"]
[2,"光通量(单颗）",">10 lm ",null,">10 lm "]
[3,"LED芯片","台湾晶元（或同档次）",null,"台湾晶元"]
[4,"CTC微光发电板(弱光测试）",{"v":0.1988,"d":"19.88%"},null,{"v":0.1988,"d":"19.88%"}]
[5,"CTC微光发电板(强光测试）","24-25%",null,"24-25%"]
[6,"电压","12V",null,"24V"]
[7,"锂电池","30Ah",null,"40Ah"]
[8,"色温","3000K-9000K",null,"3000K-9000K"]
[9,"显色指数","75-85",null,"75-85"]
[10,"每天照明时间","12-15h",null,"12-15h"]
[11,"抗阴雨天数","365天",null,"365天"]
[12,"使用环境","﹣40℃-70℃",null,"﹣40℃-70℃"]
[13,"灯具材质","全铝合金",null,"全铝合金"]
[14,"锂电池寿命","3-5年",null,"3-5年"]
[15,"光源寿命","＞80000小时",null,"＞80000小时"]
[16,"控制器防护等级","IP67",null,"IP67"]
[17,"整灯防护等级","IP65",null,"IP65"]
[18,"灯柱规格","高度6米，上下口径60*140mm,壁厚3mm，出臂1米，直径60mm，厚2.5mm，法兰260*260*12mm，灯杆材质为热镀锌钢管 ",null,"高度9米，灯杆臂厚4mm，上150*150mm，下200*200mm，法兰400*400mm，出臂1.2m，灯杆材质为热镀锌钢管"]
["1.产品价格为到最终需方指定现场价格(含运保费)，包含从安装验收合格后起24个月的保修期费用。"]
[]
["灯具图样确认表"]
["序号","类型","单价","图片","备注"]
[1,"单臂6m高","灯杆为圆管",null,"灯杆样式为统一样式，双臂为意向效果图，实际使用参照单臂样式"]
[2,"双臂6m高","灯杆为圆管；\n双臂路灯为两盏60W灯具"]
[3,"单臂9m高","灯杆为方管"]

{"sheet":"Sheet3","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}